
1：Please upgrade firmware first with → Update FirmwareGD-77\_V2.6.8


2：And then install the new software → Update Software GD-77\_V1.1.12

3：New firmware V2.6.8 must be used with new software V1.1.12.


4：128 RX Group List activation ！！

1) Read frequency 

2) Manual input RX Group



3) Don't do anything else and write frequency directly.



4) Activation completed. Then you can use and test if it can work properly.